|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **F2 Unit 41– Prescription and Implementation Guide** | | | | **WRITTEN BY: *K. Zimlinghaus*** | |
| RX DATE: 10/12/2017 | **DIAGNOSIS DATE: 10/10/2017** | | | **CERTIFIED BY: *K. Zimlinghaus*** | |
| **BASE FISCAL YEAR: 2018** | **NEPA ACRES: 29** | | **UNIT ACRES: 20** | |  |
| **ENVIRONMENTAL ANALYSIS:**  **Forsythe II Project** | | **DECISION DATE: 7/10/2017** | | | **EXISTING BASAL AREA = ~10 sq. ft./acre** |

|  |  |  |  |
| --- | --- | --- | --- |
| **ACTIVITY** | **TIME** | **AC** | **DESCRIPTION, MARKING GUIDES, MONITORING, ETC.** |
| Meadow/ Shrubland Restoration | 2018 | 20 | Objectives   * Reduce the severity and intensity of a wildfire within the WUI. * Restore ponderosa pine/mixed conifer stands, aspen, and meadow/shrublands toward their characteristic species composition, structure, and spatial patterns in order to increase resistance and resiliency to future natural disturbance. * Old growth tree component: retain ponderosa pine greater than 14” DBH or ponderosa pine greater than 10” DBH with flat top crowns and/or bark that is orange over 50% of the bole of the tree. NOTE: Flammulated owl habitat; retain all conifers over 12” DBH.   Cutting Guides   * Cut all conifers regardless of species up to 12” DBH. EXCEPTION: Retain at least one conifer < 12” DBH around picnic sites to provide future shading opportunities. * Retain all limber pine that do not pose a safety hazard. * Retain 1-3 Rocky Mountain juniper per acre where a given acre has 2 or more trees. * Retain snags (dead trees) >12” DBH. * Retain all existing down woody material 5” in diameter or greater within and up to 100 feet of riparian areas for * prebles habitat. |
| Slash Treatment All Units | 2018 | 20 | * Hand pile existing and activity slash material 1” to 6” diameter and 2’ or longer. Any slash that must be moved more than 50’ to meet minimum required pile size may be lopped and scattered to a maximum depth of 18”. * All treated material shall not be left beneath or within 10’ of the dripline of a retained tree. * Piles should be at least 6’ x 6’ in diameter, 15’ apart, & 10’ from residual tree boles. Cut conifers in order to create piles when needed. * Treated bole wood 6” in diameter or greater must be scattered and be in contact with the ground. Individual boles of 8” or greater must be bucked into 4’ lengths beginning at the large end. * Pull back slash and construct piles at least 50’ from any infrastructure and private property boundaries. * Retain an average of 2 piles per acre for wildlife habitat, including any piles remaining from previous vegetation treatment, distributed randomly throughout the unit. * In aspen clone aggregations, construct piles outside of the aspen perimeter if enough material exists to establish the minimum pile size; otherwise, lop and scatter material to a height not greater than 18” from ground level. * Piles must be constructed a minimum of 100’ from all power lines. |

|  |  |
| --- | --- |
| **BOUNDARY DESIGNATION AND TREE MARK** | * + Boundary trees marked with orange flagging and painted in orange. Each exterior boundary tree will be flagged with a piece of flagging wrapped around the bole of the tree at eye level, or a strip of flagging hanging from a branch.   + This is a leave-tree mark; leave-trees will be designated with 4 dots of orange paint around the bole of the tree and a butt mark. |
| **TIMING RESTRICTIONS** | * No operations from May 1 through August 10 in flammulated owl territories. * Raptor nest areas, including species-specific buffers, will generally have no treatment activity from March 1 through September 15, depending on species, or until determined unoccupied by the wildlife biologist. Access through buffers during this period will be assessed by the wildlife biologist. * No operations from December 1 through April 30 for elk, unless determined appropriate to treat by the wildlife biologist. * Piles outside the 100 foot riparian buffer but within 328 feet of the stream channel may only be burned between November 1 and April 30. * Project operations will not be conducted on Memorial Day, 4th of July and Labor Day holiday weekends and on Sundays. Operating time for heavy equipment and chainsaws shall be limited to the hours of 7am to 7pm. |
| **FOR MORE INFO:** | Forsythe II Project EA |